Each Wilkhahn Revit Family includes specific usage instructions under the 'Floor Plans – Ref. Level_Instructions' view

> Instructions for Utilizing the Revit Type Catalogue (.txt files that accompany each Wilkhahn .rfa file)
	1.) In a Revit project or template, click Insert tabLoad From Library panel (Load Family)
	2.) Navigate to the directory containing the Wilkhahn family you want to open
	3.) Select the Wilkhahn family (.rfa file) to load
		**The Type Catalog displays
	5.) In the Type column of the Type Catalog, select the family type or types to load.
		**You can select multiple types by pressing Ctrl during selection. You can also narrow the range of search items by selecting specific parameters from the list at the top of each column.

	6.) Click Open.

> Instructions for Utilizing Material Swatches:
In order to utilise the Wilkhahn default materials you will need to 'Copy & Paste' the material texture swatches into the following Revit root material library directory. Note: your material location may vary depending on your Revit version, computer/server setup and permissions. C:\Program Files (x86)\Common Files\Autodesk Shared\Materials\Textures\3\Mats

> Contact WILKHAHN to confirm feasibility of design variations outside the scope of this Revit Family

> Wilkhahn US Contact Information:	
	Contact_Phone:	+1 (212) 229-9455 (Customer Service)
	Contact_E-Mail:	sales@wilkhahn.com

> Disclaimer:
	Due to ongoing product development and manufacturing evolution, product details are subject to change without notice.
	Please refer to product technical data sheets on www.wilkhahn.com for the most current product information.
	Please allow a +/- 5mm tolerance for dimensions and set-outs shown in product literature.
	© WILKHAHN 2016